**DQMusicBox: How to prepare the micro-SD card image**

6 January 2019

# Introduction

This document describes how to create a DQMusicBox system image – a .img file. I (Ross) am probably the only person that needs this document. Mostly people making a DQMusicBox will use the fruit (the .img file) of the process described here -- you don’t need to create your own custom .img file unless you really want to. At the time of this writing, there are two versions of the software. This version uses a USB DAC and a newer method for USB drive automounting.

# No warranty

USE THESE DQMUSICBOX PLANS AND SYSTEM AT YOUR OWN RISK. THE DQMUSICBOX PLANS ARE PROVIDED AS IS WITHOUT WARRANTY OF ANY KIND EITHER EXPRESSED OR IMPLIED, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE. THE ENTIRE RISK AS TO THE QUALITY AND PERFORMANCE OF THE PLANS AND SYSTEM IS WITH YOU. SHOULD THE PLANS OR SYSTEM PROVE DEFECTIVE, YOU ASSUME THE COST OF ALL NECESSARY SERVICING, REPAIR OR CORRECTION. IN NO EVENT WILL ANY PARTY BE LIABLE TO YOU FOR DAMAGES, INCLUDING ANY GENERAL, SPECIAL, INCIDENTAL OR CONSEQUENTIAL DAMAGES ARISING OUT OF THE USE OR INABILITY TO USE THE PLANS OR SYSTEM.

# Prepare the disk image

This is a record of how I created the disk image. You only need to read this information if you wish to do your own OS configuration.

## Install DietPi on 4GB micro-SD card

Install DietPi i.e. follow these instructions: <http://dietpi.com/phpbb/viewtopic.php?f=8&t=9#p9>. I installed v140. I used [balenaEtcher](https://etcher.io/) (free) to write the disk image to the micro-SD card. This may take a while as the system updates itself.

## Boot & configure DietPi

Put the Pi on Ethernet. Move the micro-SD card to the Pi, boot DietPi. After a build process, you will be prompted to make some choices.  
  
DietPi-Config

|  |
| --- |
| Audio Options: Soundcard : usb-dac |

Software Optimized

|  |
| --- |
| Hardware Projects : RPi.GPIO [Install] |

Software Additional

|  |
| --- |
| System : ALSA  Development : Git Client |

Install

|  |
| --- |
| Install |

Software will be installed. Then your Pi will then reboot

## Install VLC (music player)

|  |
| --- |
| sudo apt-get install vlc-nox |

## adduser pi

|  |
| --- |
| sudo adduser pi |

## Install/clone dqmusicbox, enable

|  |
| --- |
| cd /home/pi  git clone <https://github.com/rosswesleyporter/dqmusicbox/>  sudo chmod 755 dqmusicbox/bin/dqmusicbox\_usb.py |

## Install Python bindings for VLC

|  |
| --- |
| cd /home/pi  sudo git clone https://github.com/oaubert/python-vlc  cp python-vlc/generated/2.2/vlc.py dqmusicbox/bin  chmod 755 dqmusicbox/bin/vlc.py |

## Add shell script to automatically start the musicbox

|  |
| --- |
| cd /home/pi  sudo cp dqmusicbox/bin/dqmusicbox\_usb.sh /etc/init.d  sudo chmod 755 /etc/init.d/dqmusicbox\_usb.sh  sudo update-rc.d dqmusicbox\_usb.sh defaults |

For more information, see Stephen Christopher Phillips’ [terrific page](http://blog.scphillips.com/posts/2013/07/getting-a-python-script-to-run-in-the-background-as-a-service-on-boot/).

## Configure such that USB drives mount automatically

The instructions below are from [pauliucxz](https://raspberrypi.stackexchange.com/users/66022/pauliucxz) in [StackExchange 66169](https://raspberrypi.stackexchange.com/questions/66169/auto-mount-usb-stick-on-plug-in-without-uuid), preserved below for clarity. I am quite thankful for that answer. The first USB drive will automatically mount as /media/usb1.

Install pmount

|  |
| --- |
| sudo apt-get install pmount |

Specify a udev rule by creating file /etc/udev/rules.d/usbstick.rules

|  |
| --- |
| ACTION=="add", KERNEL=="sd[a-z][0-9]", TAG+="systemd", ENV{SYSTEMD\_WANTS}="usbstick-handler@%k" |

Configure a system service by creating file /lib/systemd/system/usbstick-handler@.service

|  |
| --- |
| [Unit]  Description=Mount USB sticks  BindsTo=dev-%i.device  After=dev-%i.device  [Service]  Type=oneshot  RemainAfterExit=yes  ExecStart=/usr/local/bin/cpmount /dev/%I  ExecStop=/usr/bin/pumount /dev/%I |

Create the mount script file /usr/local/bin/cpmount

|  |
| --- |
| #!/bin/bash  if mountpoint -q /media/usb1  then  if mountpoint -q /media/usb2  then  if mountpoint -q /media/usb3  then  if mountpoint -1 /media/usb4  then  echo "No mountpoints available!"  #You can add more if you need  else  /usr/bin/pmount --umask 000 --noatime -w --sync $1 usb4  fi  else  /usr/bin/pmount --umask 000 --noatime -w --sync $1 usb3  fi  else  /usr/bin/pmount --umask 000 --noatime -w --sync $1 usb2  fi  else  /usr/bin/pmount --umask 000 --noatime -w --sync $1 usb1  fi |

Make the script executable

|  |
| --- |
| sudo chmod 755 /usr/local/bin/cpmount |

## Shutdown, unplug

|  |
| --- |
| sudo shutdown -h now |

Then unplug the Pi

## Insert USB drive

Once Pi is off, insert USB drive. Then plug the Pi back in.

## Test

Make sure the music plays…

## Shutdown

Provided that the reboot went well, shutdown:

|  |
| --- |
| sudo shutdown –h now |

Then remove the micro-SD card.

## Use Win32DiskImager to create the master image

Remove the micro-SD card from your Pi and place in the card reader of your computer. Use Win32DiskImager to create an image of DQMusicBox that you just nicely configured.